**9**. THIS SECTION TO BE COMPLETED BY ALL APPLICANTS **UNLESS** AOC/OPERATIONS SPECIFICATIONS ARE ICAO ANNEX 6 APPENDIX 6 COMPLIANT.

|  |
| --- |
| ***OPERATIONS SPECIFICATIONS****(subject to the approved conditions in the operations manual)* |
| ***ISSUING AUTHORITY CONTACT DETAILS (FOREIGN STATE OF OPERATOR)****Telephone: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Fax: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ E-mail: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_* |
| *Aircraft Registration / Model:* |
| *Type of Operation: Commercial Air Transport*  *Passengers Cargo Others: \_\_\_\_\_\_\_\_\_\_\_\_\_* |
| *Area(s) of Operations: List the geographical area(s) of authorized operation (by geographical coordinates or specific routes, flight information region or national or regional boundaries)* |
| *Special Limitations (List the applicable special limitations (e.g. VFR only, day only).* |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***Special Authorizations*** | ***Yes*** | ***No*** | ***Specific approvals*** | ***Remarks***  |
| ***Dangerous Goods*** *Operator’s Ops Specs Ref :***\_\_\_\_\_** |  |  |  |  |
| ***Low visibility operations**** ***Approach and landing***
* ***Take-off***

*Operator’s Ops Specs Ref: \_\_\_\_\_* |  |  | ***CAT: \_\_\_\_\_ RVR: \_\_\_\_\_ m*** ***DH: \_\_\_\_\_ ft******RVR3: \_\_\_\_\_ m*** | Insert the applicable precision approach category (CAT I, II, IIIA, IIIB or IIIC), CAT II and above required separate approval.Insert the approved minimum take-off RVR in metres |
| ***RVSM ☐ N/A****Operator’s Ops Specs Ref: \_\_\_\_\_* |  |  |  | Not applicable (N/A)” box may be checked only if the aircraft maximum ceiling is below FL 290. |
| ***ETOPS ☐ N/A****Operator’s Ops Specs Ref: \_\_\_\_\_* |  |  | ***Maximum diversion time:*** ***\_\_\_\_\_ minutes***The threshold distance may also be listed (in NM), as well as the engine type | (ETOPS) currently applies only to twin-engine aircraft. “Not applicable (N/A)” box may be checked if the aircraft model has more than 2 engines. |
| ***Navigation specifications*** ***for PBN operations****Operator’s Ops Specs Ref: \_\_\_\_\_* |  |  |  | *One line is used for each PBN specification authorization (e.g. RNAV 10, RNAV 1, RNP 4), with appropriate limitations or conditions listed in the “Specific Approvals” and/or “Remarks” columns.**Limitations, conditions and regulatory basis for operational approval associated with the performance-based navigation specifications (e.g. GNSS, DME/DME/IRU). Information on performance-based navigation, and guidance concerning the implementation and operational approval process, are contained in the* Performance-based Navigation (PBN) Manual *(Doc 9613).* |
|  ***Continuing airworthiness****Operator’s Ops Specs Ref: \_\_\_\_\_* |  |  |  | *Insert the name of the organization or person responsible for ensuring that the continuing airworthiness of the aircraft is maintained and the Regulation that requires the work, i.e. within the AOC regulation* |
| ***Other****Operator’s Ops Specs Ref: \_\_\_\_\_* |  |  |  | *Other authorizations or data can be entered here* |